Switching Network Devices Network devices can be disabled so they are not operable or enabled so they are operable. Automatic Network Switch This useful function automatically connects to a wireless LAN when the wired LAN cable is disconnected and automatically connects to a wired LAN when the cable is reconnected. In addition, this function automatically connects to a dial-up connection when both the wired LAN and wireless LAN are disconnected. Automatic Profile Switch This function can be used to automatically switch profiles to match the connected wireless LAN network (SSID). Program Start-up This function can be used to configure the program you want to start after a profile is selected. System Tray Icon Shortcuts These shortcuts enable you to easily connect to dial-up, Virtual Private Network (VPN), or broadband connection service. Using a Wireless LAN Access Area You can easily connect to a wireless LAN access area by simply connecting to the appropriate SSID and clicking the notification window. (You must have an account with a service provider before you can use this function to connect to a wireless LAN access area.) Turning Bluetooth On/Off This enables you to turn the Bluetooth power on or off. Create profiles with the profile wizard Create a profile using setup items manually with the profile wizard. Import/Export Profiles Create a profile by import / export file. Using Quick Connect to Connect a Wireless LAN Projector This function can be used to instantaneously start up a Toshiba wireless LAN projector from the connection setup screen on the projector or the connection utility on the PC. Using Quick Connect for ad hoc network Direct Link TOSHIBA Device is used in an environment where an Access Point is not present. This feature configures the wireless PC quickly in ad hoc (peer-to-peer) mode. Use setting dialogs Device, detail and option settings can be changed.