Using Quick Connect for ad hoc network
Direct Link TOSHIBA Device is used in an environment where an Access Point is not present. This feature configures the wireless PC quickly in ad hoc (peer-to-peer) mode and starts SUMMIT.
Set up the Wireless network device Connecting to the Toshiba Device Disconnect the Toshiba Device

1 | Set up the Wireless network device

Check the setting of the wireless network device used to connect the PC to the Toshiba Device. The setting on the wireless network device must match the setting on the Toshiba Device in order to connect the PC to Toshiba Device. As default settings, Network Name (SSID) is set to ConfigFree Link. If any changes are made to the Toshiba Device settings, be sure to make the same changes to the settings on the wireless network device.

| Opening Quick Connect properties
| Left-click the icon in the system tray.
| Move the cursor to Direct Link Toshiba Device.
| Click Settings. Quick Connect settings screen is displayed.
When the 'Add' button is clicked the following SSID setting screen is displayed. The SSID, the WEP key, and the TCP/IP settings can be modified.

| Matching the Settings on the Toshiba Device
| Set Network Name (SSID).
| Wireless Network Key (WEP) If Data Encryption (WEP enabled) is enabled, set the following items. - Data Encryption (WEP enabled) Moreover, it changes into the IP address specified after setting change of wireless LAN.
| Click OK.

2 | Connecting to the Toshiba Device

| Connecting to the Toshiba Device
| Left-click the icon in the system tray.
| Move the cursor to Direct Link Toshiba Device.
| Click ConfigFree Link.
| SUMMIT Starts
The wireless LAN settings change to the specified wireless LAN device settings.

3 | Disconnect the Toshiba Device

| Disconnect the Toshiba Device
| Left-click the icon in the system tray.
| Move the cursor to Direct Link Toshiba Device.
| "ConfigFree Link" currently checked is chosen.